PAVEMENT

|  |  |
| --- | --- |
| Pothole | Single pothole, area for patching, rigid or flexible pavements |
| Outside Qtr | Settlement on the outside quarter of a flexible pavement |
| High edge | Buildup on/along roadway edge |
| Low edge | Loss of roadway edge/drop-off |
| Wheel rut | Rutted area in flexible pavements |
| Failures | Failed area in rigid or flexible pavements |
| Spot Mill | Bump or hump, spot area to be milled |
| Sweeping | Area to be swept |
| CTB | Concrete Traffic Barrier damage or other related work |
| Raveling | Aggregate separation in asphalt pavements |
| Bleeding | Bleeding and or flushed area in asphalt pavements |
| Railroad | Approaches, crossings, etc. |

TRAFFIC

|  |  |
| --- | --- |
| Striping | All striping and graphic pavement markings |
| Delineation | All delineation, post or rail mounted, spots or sections |
| Signs | All traffic signs |
| Signals | Traffic signals and appurtenances |
| Safety Lighting | Luminaires, high mast and underpass lighting, etc. |
| Attenuators | Crash barrier |
| Flashing beacons | School zone, warning lights, etc. |
| RPM’s | Raised pavement markers |
| Mailbox | And/or supports |
| Encroachment | Illegal signs and other unauthorized ROW use |
| Graffiti | Graffiti for removal, documentation |

ROADSIDE

|  |  |
| --- | --- |
| Mowing | Spot areas needing mowing |
| Herbicide | Area/spot needing chemical vegetation control/pruning |
| Trees | Trees for removal/trimming, etc., |
| Litter | Illegal dumpsites, other spot litter/debris issues |
| Guardrail | Damaged guardrail, end treatments, rail upgrades, etc. |
| Cable Barrier | Damaged cable median barrier |
| Erosion | Eroded areas needing repair |
| Curb | Damaged curb section |
| Inlet | Curb inlets and other drain inlets needing repair/cleaning |
| Drainage | Ditches, culverts, drift, etc. |
| Sight Visibility | Area that has sight visibility issues |
| Side Road | Side road approaches we maintain |

STRUCTURES

|  |  |
| --- | --- |
| Decks | Bridge deck |
| Joints | Bridge joints |
| Rails | Bridge rail damage/upgrade |
| Debris | Debris on deck/caps/structure |
| Drift | Drift needing removal from bridge channel |
| Approach slab | Settlement, ride, and/or damaged bridge approach slab |
| Spalling | Concrete spalling, decks and structure |
| Impact damage | Impact damage to structure |
| S.E.T’s | Safety end treatments/pipe runners on culverts and bridge culverts |
| Slope failed | Failed bridge/overpass slope |
| Rip rap | Concrete lined slopes/ditches needing repair or maintenance |
| Backwall | Damaged bridge abutment back walls |
| Fenders | Bridge protection systems |

OTHER

|  |  |
| --- | --- |
| Incident | Monitor traffic control, assist with cleanup, damage assessments |
| Work request | Meet customers, assess work needs, develop plan |
| Checked okay | Verify standards met, assess conditions |
| Driveways | Permit requests, measurements, inspections |
| Boat ramp | Boat ramp needing maintenance or repairs |
| Picnic area | Picnic area maintenance or repairs |
| Rest area | Rest area maintenance or repairs |

PLANNING

|  |  |
| --- | --- |
| Seal coat | Roadway section to be sealed |
| Overlay | Roadway section to be overlaid |
| Milling | Roadway section to be milled |
| Joint seal | Rigid pavement section to have the joints sealed |
| Crack seal | Flexible or rigid pavement section to have cracks sealed |
| Fog seal | Roadway section to be fog sealed |
| Conc. repair | Spot area or roadway section for repairs, rigid pavements |
| Widening | Area or section to be widened, rigid or flexible |
| Other project | Use for other planned projects, describe using notes function |